The YSI 6600 V2 data sonde is the most comprehensive water quality monitoring equipment available with simultaneous measurement of conductivity (salinity), temperature, depth or level, pH/ORP. The 6600 V2-4 also measures these parameters: dissolved oxygen, turbidity, chlorophyll, and blue-green algae; the V2-2 measures two of the four parameters simultaneously. Additional calculated parameters include total dissolved solids, resistivity, and specific conductance. <br/><br/>
For more information see help file: Field Logger Import <br/>
For an example file: Tutor > Sensor Examples > 6600YSI <br/>
Manufacturer Reference: <a href="https://www.ysi.com/6600-V2-4 "> YSI_6600V2 </a>
