The TROLL 9500 water quality instrument accommodates the following sensors: <br/>
Rugged Dissolved Oxygen (RDO) sensor <br/>
Clark cell DO sensor <br/>
Conductivity in both low and high ranges <br/>
Ion-selective electrodes - Ammonia, chloride, and nitrate <br/>
pH <br/>
pH/ORP <br/>
Pressure <br/>
Turbidity, with or without a wiper <br/><br/>
The data will be imported to the In-Situ_TROLL9500 tab in EDGE <br/><br/>
For more information see help file: In-situ troll loggers <br/>
For an example file: Tutor > Sensor Examples > Troll9500 <br/>
