The vented (gauged) Level TROLL 500 measures and records water level, pressure, and temperature. The logger is available in six different pressure ranges—from 5 psig to 500 psig. The Level TROLL 500 automatically compensates for barometric pressure, which significantly reduces time required to post process data. <br/>
This import also supports the TROLL 100, 300 and 700. <br/><br/>
For more information see help file: Live Logger Import <br/>
For an Example File : Tutor > Sensor Examples > Troll500   (note: also have examples of 100,300 and 700) <br/>
Manufacturer Reference: <a href="https://in-situ.com/products/water-level-monitoring/level-troll-500-data-logger/"> In-Situ-Level-500 </a>