The YSI Model 556 simultaneously measures numerous water quality parameters including temperature, conductivity, salinity, dissolved oxygen, pH, and ORP. <br/><br/>
For more information see help file: Field Logger Import <br/>
For an example file: Tutor > Sensor Examples > ProPlus&556 <br/>
Manufacturer Reference: <a href="https://www.ysi.com/556 "> YSI_556 </a>
