The Levelogger Gold is a self contained water level datalogger, which is completely designed, developed and manufactured in-house, in the tradition of all Solinst high quality products. The Levelogger Gold uses infra-red data transfer, providing the flexibility of simple wireline installation, or using a Direct Read Cable to surface. The Levelogger Gold includes a pressure transducer, temperature sensor, 10 year lithium battery (based on 1 reading per minute), and internal datalogger with a capacity of 40,000 temperature and groundwater level data points. <br/><br/>
For more information see help file: Solinst & Live Logger Import <br/>
For an example file: Tutors > Sensor Examples > LevelLogger(Gold) <br/>
Manufacturer Reference: <a href="https://www.solinst.com/products/dataloggers-and-telemetry/3001-levelogger-series/operating-instructions/user-guide/1-introduction/1-1-7-levelogger-gold.php"> Solinst_Levelogger_Gold </a>
