# https://www.ysi.com/File%20Library/Documents/Manuals/069300-YSI-6-Series-Manual-RevJ.pdf, Version 5.10
# Appendix N: Parameter Codes

# Parameter Id, EarthSoft.Live.Sensors.Common.Enums.ParameterUuid

# 51, Date
# 52, Date
# 53, Date
# 153, Date
# 54, Time

1, Temperature
2, Temperature
3, Temperature

6, Specific_Conductivity
7, Specific_Conductivity

4, Conductivity
5, Conductivity

9, Resistivity
8, Resistivity
94, Resistivity

10, TDS
95, TDS

12, Salinity

14, DO # DOsat
200, DO # DOsat
15, DO
# 96, DOchrg

# 209, Cl2
# 210, Cl2chrg

20, Pressure
104, Pressure
21, Pressure
111, Pressure

22, Depth
23, Depth

118, Flow
166, Flow
167, Flow
168, Flow
164, Flow
119, Flow
165, Flow
120, Flow
121, Flow
169, Flow
170, Flow
171, Flow
122, Flow
172, Flow

# 123, Volume
# 124, Volume
# 173, Volume
# 125, Volume
# 126, Volume
# 174, Volume

18, pH
17, pH

19, ORP

48, NH4__N # NH4+ N
108, NH4__N # NH4+ N

47, NH3_N # NH3 N
106, NO3__N # NO3- N
101, NO3__N # NO3- N

112, Cl_ # Cl-
145, Cl_ # Cl-

# Output from special photosynthetically active radiation sensor in mv, or Photon Flux Density in umoles/sec/m2.
# 201, PAR1
# 202, PAR2

# 'turbid NTU' = 6026 sensor, and 'turbid+ NTU' = 6136 sensor. The different designations are designed to differentiate the data from the two sensors types in later analysis.
37, Turbidity
203, Turbidity # Turbidity+

193, Chlorophyll
194, Chlorophyll
204, Rhodamine_WT

211, DO # ODOsat
214, DO # ODOsat
212, DO # ODO

215, BGA_PC
216, BGA_PC

217, BGA_PE
218, BGA_PE

# 98, Gnd
# 99, Scale
# 100, Prescmp
32, Water_Density
28, Battery_Voltage
