The GEM 2000 was designed by CES-LANDTEC specifically for use on landfills to monitor landfill gas (LFG) extraction systems, flares, and migration control systems. <br/>
The GEM 2000 samples and analyzes the Methane, Carbon Dioxide and Oxygen content of landfill gas. The easy-to-read LCD screen shows the results as percentages of CH4, CO2, O2 and “balance” gas. The GEM 2000 calculates and displays gas flow rate. It also measures and displays Btu content, temperature (w/optional probe), relative and atmospheric pressures and CH4 LEL (Lower Explosive Limit). <br/>
<br/>
For more information see help file: Landtec GEM 2000 <br/>
For an example file: Tutor > Sensor Examples > LandtecGem200 <br/>
Manufacturer Reference: <a href="http://www.landtecna.com/wp-content/uploads/2015/11/GEM2000-Pre-SN-10000-Manual-Rev-Dec-2010-1.pdf"> Landtec </a>



